**Known Issues**

1. Although steps have been taken to reduce nitrate volatilization from Teflon filters, it is likely that some loss occurs during collection, transport, and handling. Thus, nitrate concentrations should be treated as qualitative. See Snider et al. 2015 in the publications section.